	Datasheet for brake calculation for centre axle trailer

Request back to: Brakecalculation.dehe@safholland.com

	
  

	Manufacturer:      
Type of vehicle:       
	Country of homologation:        
Approval acc. to:         

	
|_|

	
	Technical data:
	Laden:
	Unladen:

	
	
	Gross veh. weight P:
	           kg
	           kg

	|_|
	
	Axle load PR 1:
Axle load PR 2:
Axle load PR 3:
Axle load PR 4:
	                  kg 
                  kg 
                  kg 
                  kg
	           kg
           kg
           kg
           kg

	|_|
	
	Axle load  PR:
	      kg
	      kg

	
	
	Tyre, min:      

Rdyn. /Rstat.:       mm /       mm

Tyre, max:      

Rdyn. /Rstat.:       mm /       mm

	|_|
	

	

	vmax. [km/h] for agriculture trailers only:
|_| ≤25    |_| ≤30    |_| ≤40    |_| ≤ 60    |_| > 60

	Service brake system with:

|_| EB+4.0  |_| EB+Gen3               S /       M
|_| ABS 4.0                                     S /       M
|_| UABS                                        S /       M
|_| without ABS or EBS

Further valves:

[bookmark: Kontrollkästchen2]|_| TrCM / TrCM+    |_| TEM    |_| TEM+    |_| REV
[bookmark: Kontrollkästchen1][bookmark: Kontrollkästchen11]|_| LSV   |_| with light/ laden valve

	Parking brake system:

|_| with spring brakes on which axles:      

No.:         Type:      

	
	or mechanical hand brake system:

|_| with hand screw type: Manufacturer      
Type:      
Test report number:      

	Axles / Foundation brakes:
	1. Axle:
	2. Axle:
	3. Axle:
	4. Axle:
	Brake actuator: 

No. per axle:

|_| 1      |_| 2


	Manufacturer of axles / axle type:
	     
	     
	     
	     
	

	Manufacturer of brakes / Type:
Test report e.g. TDB-No.:
	     
     
	     
     
	     
     
	     
     
	Remark:
     

	Possible lever lengths:
	     
	     
	     
	     
	

	Brake chamber manufacturer / -type
Test report e.g. TDB-No.:
	     
     
	     
     
	     
     
	     
     
	

	Suspension unit

	[bookmark: Kontrollkästchen3][bookmark: Kontrollkästchen4][bookmark: Kontrollkästchen5]|_|  Mechanical, balanced suspension during braking cond.  |_| yes  |_| no          (VB or W/GW etc.)

Manufacturer / Type:              spring deflection, laden to unladen:  Δfs       mm

     

	
	[bookmark: Kontrollkästchen6]|_|  Air suspension – bellow pressures: laden:       bar, unladen:       bar

Manufacturer:       Type:      

[bookmark: Kontrollkästchen14]|_| Axle lift on axle(s):             |_| Self steering axle(s):      


	Contact:      
	Date:                                
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